## Item specifics

|  |  |  |  |
| --- | --- | --- | --- |
| Condition: | New: A brand-new, unused, unopened, undamaged item in its original packaging (where packaging is ... [Read more](javascript:;) | To Fit: | Ham Radio Transceiver |
| Type: | DIGITAL INTERFACE | Country/Region of Manufacture: | United States |
| MPN: | Easy Digi USB Complete with cables | Compatible Brand: | Universal |
| Brand: | EASY DIGI™ | Country of Manufacture: | United States |
| UPC: | Does not apply |  |  |

**UNIVERSAL EASY DIGI™ USB W/AUDIO CABLES**

**Easy Digi does NOT do CAT control**

Please look at the third picture. If your radio is NOT listed there then do NOT order this item.

You will need to order eBay item# 32411749167 and send me a message telling me what radio you want it wired for.

WIN-XP, VISTA, WIN-7, WIN-10, LINUX

WSJT-X, FLDIGI, FT-8, PSK, Many other sound card based modes

**Includes two (2) 1 meter long audio cables.**

**This Easy Digi™ USB digital interface plugs directly into an open USB port on your computer!**

**In most cases, it will go out to the internet and find it’s drivers, install them, and tell you it’s ready to go!**

**A single driver CD is included!**

**We’ve tested it on XP, XP-PRO, VISTA, WIN-7and WIN-10 with excellent results.**

**This interface is configured to work with a large variety of radios as is with nothing else required.**

**While we have sold several thousand of the previous versions, this is a major step forward for our little interface with a minor step in pricing.**

**Nothing new about this technology, it consists of two 600 ohm line transformers for audio input and output from your pc to your transceiver, and an opto-coupled push to talk circuit that works off of a USB port on your computer.**

* **Transformer coupled audio eliminates ground loops and AC hum on your signal**
* **Opto Coupled push to talk circuit also eliminates ground loops and false triggering of your PTT lines.**
* **Very small size, only 3 13/16”L  x 1 9/16”W  x 3/4” H, can be mounted using the built in mounting tabs in just about any convenient location.**
* **Case made of durable ABS Plastic for long life.**
* **Built in USB Serial adapter, connects to USB port on any PC**
* **Weighs less than 3 ounces**
* **High quality FR-4 double sided, solder masked, silk screened Printed Circuit Board**
* **Compatible with most modern ham radio transceivers.**

**Preconfigured to work with the following radios:  
ALINCO DR-735**

**YEASU:**

**FT-450, FT-817, FT-818, FT-857, FT-891, FT-897**

**FT-950, FT-991, FT-1500, FT-7100, FT-7800**

**FT-7900, FT-8100, FT-8500, FT-8800, FT-8900**

**FTDX-1200, FTDX-3000**

**KENWOOD**

**TS-480, TS-480HX, TM-733, TMD-700, TMD-710**

**TMG-707, TM-V7, TM-V71**

**ICOM**

**IC-746 PRO (VHF/UHF only) , IC-7000, IC-7100**

**Please see our “other items” for other versions of this interface.**

**Order yours today!**

**Works with all windows based laptops and desktops, xp, xp-pro, vista, win-7, win-8, win-10, and Linux!**

**When you order, usually at the bottom of the listing page is a link to ask a question.**

**Ships worldwide and usually ships within 48 hours of payment except for weekends and holidays.**